**HAP Placement in Wireless Powered Communication Networks Using Deep Learning**

**Hong-Sik Kim, Hanyang University, Department of Computer Software**

**Abstract**

HAP (Hybrid Access Point) is a node in Wireless Powered Communication Networks (WPCN) that can distribute energy to each wireless device and also can receive information from these devices. For efficient use of network, we should maximize the throughput of the network. There are two kinds of metrics for throughput, that is, sum throughput and common throughput, each is the sum and minimum value of throughput between a HAP and each wireless device, respectively. There are two types of throughput maximization problems, sum throughput maximization and common throughput maximization. In this paper, we discuss about the latter. We used deep learning methodology to maximize common throughput. Our study implies that deep learning can be applied to maximize a simple function of common throughput maximization, which is a convex function or a combination of a few convex functions, and shows better performance than mathematical methodologies.

**1. Introduction**

In WPCN, there is Access Point (AP) mechanism **[1]** which contains energy nodes (EN), wireless devices (WD) and access points (AP). First, energy nodes send energy to each wireless devices. When ENs receive the energy, it sends information to APs using the energy. That is, ENs send energy to WDs and WDs send information to APs. We can encapsulate AP and EN into Hybrid Access Point (HAP) and so can describe HAP mechanism. In this mechanism, the HAP sends energy to each WD, and each WD sends information to the HAP. The HAP allocate time for sending energy to each WD to itself, and for sending information to each WDs, so time allocation to itself and each WDs is also an important issue.

Because the distance between the HAP and each WD is different among each WD, there is energy efficiency gap between the WDs caused by the difference of throughput for each WD. That is, a WD near to the HAP receives more energy and uses less energy to transmit information, and another WD far from the HAP receives less energy but uses more energy to transmit information. To solve this unfairness problem, the worst case, a WD which receives least energy and uses most energy, is very important. For this case, we use the concept of common throughput which is the minimum value of throughput among the throughput values of each WD, and we concentrate on maximizing the common throughput value in the WPCN environment.

This paper introduces a methodology to place HAPs in WPCN environment to maximize common throughput when time allocation is optimized, by using deep learning, and shows that this methodology is meaningful to solve this problem and shows better performance than the mathematical methodology already studied.


**2. Related Works**

In **[2]**, Suzhi Bi and Rui Zhang researched about the placement optimization of Energy and Information Access Point in WPCN using Bi-section search method, Greedy algorithm, Trial-and-error method, and alternating method for joint AP-EN placement. There can be more than 1 HAPs WDs in the supposed environment of this paper. Its methodology is repeatedly adding HAPs and check if each WD satisfies conditions in the environment.

**3. HAP Placement Model**



**3.1. Overview**

**Figure 1** is the flow chart for the HAP placement model. The model is composed of three phases. Making data is the first phase to create training and test data. Training using data is the next phase to process the data to training and test data for the deep learning model, and train using the model. Finding the best point is the last phase to find the best HAP placement point using the throughput map derived by this model.



**WDs placement map** means the square map with rows and columns, and random K blocks in the map contains a WD. There are no WDs with the same position in the map. From now on, we will call this . **Throughput map** means the square map with rows and columns, and each block contains the throughput value where the HAP is located in this block of . From now on, we will call this . **Best throughput point** means the position of HAP that maximize throughput value in . we will call this .

**3.2. Making Data**


To make s where is the sum of the number of training and test maps, first define a square map with rows and columns. Then repeat placing a WD at the randomly selected point times. To make s using these s, place HAP at each point in s and compute throughput for the location of HAP and each WDs using **Algorithm 1** because throughput value is computed using **Formula (6)** in **[3]**. getThrput function finds optimal time allocation given . Because we supposed that and where is the distance from the HAP and each WD, this formula can be converted into **(1)**. To prevent divide by 0 error and consider the limit of throughput, we supposed that distance is 1.0 when actual distance is less than 1.0.

Then, because s and s are saved as text files, the model must read them before using them.

**3.3. Training Using Data**

First, make input data for training and testing based on , supposing that the number of training and testing data is and each. The model considers first maps as training data and next maps as test data. The input data is an map whose value at each block is -1 when a WD is at this block and 0 otherwise. Then make output data for training based on s corresponding to s. The output data is an map whose value at each block is processed version of the common throughput value derived by **Algorithm 1** where the HAP is at this block. The following is the processing procedure. First, find maximum throughput value for each training output map , and then divide each value , at the intersection of row and column in this map by the maximum value among these values. Last, process each value at each block using **(2)**.

Then training using input data s and corresponding output data s using the deep learning model described in **Figure 2** with Adam optimizer **[4]** with learning rate 0.0001 and 1,000 epochs.





**3.4. Finding the Best Point**

Using test input data, the model finds best point for HAP placement. For each test input data created based on in **3.3.**, input these data into the model trained in **3.3.** and get output maps corresponding to . For each value at each block in each output map is converted by **(3)** using inverse function of sigmoid function, to convert them from from into form, where is the estimated common throughput value.

Then, for each output map, the model finds maximum value among values in blocks of this map. Let’s call row and column axis of this value in the map and each, and call the maximum value . Then the row axis and column axis of optimal HAP location is computed by **(4)** and **(5)** each, and is computed by **(6)**, described in **Figure 3**.

If is greater than , moves down from original position and otherwise it moves up. Similarly, if is greater than , moves right and otherwise it moves left. Because original common throughput and can be converted into each other by just a linear transmission, there is no difference of and between when converted into and do not convert into any other form.





**4. Experiment**

**4.1. Experiment Design and Test Metrics**


**Figure 4** is the flowchart for experiment. For each optimal HAP location for each test map derived by **3.4** corresponding to s, first compute common throughput value using this point. Because we use s only for computing the difference when testing, the throughput maps as created as the output of model, called s in this section, are not equal to corresponding s. Then compare the throughput value with the maximum common throughput value in corresponding . Then the test metrics are defined as and computed using **(7)**, **(8)** and **(9)**.

means average common throughput for each test map, means maximum common throughput value for each throughput map corresponding to each test map, and means the rate between the sum of and the sum of for all test maps. It also means the rate between and . We also define performance rate as **(10)** meaning how good our methodology is compared to the methodology used in the original paper, and the original paper in **(10)** means **[2]**.

**4.2. Experiment environment**

The computer system information for our experiment is as the following. The operating system is Window 10 Pro 64bit (10.0, build 18363), system manufacturer is LG Electronics, the system model is 17ZD90N-VX5BK, the BIOS is C2ZE0160 X64, the processor is Intel® Core™ i5-1035G7 CPU @ 1.20GHz (8 CPUs), ~1.5GHz, and the memory is 16384MB RAM. The programming language is Python 3.7.4, and used NumPy, Tensorflow and Keras as libraries. You can download the experiment code written in Python from <https://github.com/WannaBeSuperteur/2020/tree/master/WPCN>.

**4.3. Experiment Result**

**Figure 5** describes and values for our methodology and the methodology in the original paper. For our methodology, value increases when the number of WDs increases and decreases when the size of maps increased, and decreases when both the number of WDs and the size of maps increased. For the methodology in the original paper, increases when both the number of WDs and the size of maps increased, and as the same as our methodology, decreases when both the number of WDs and the size of maps increased. **Figure 6** describes and values for each size and number of WDs. decreases when both the number of WDs and the size of maps increased and decreases when the size of maps increased, but has no significant correlation with the number of WDs. For small size, our methodology shows significantly better performance than the methodology in the original paper, but for 16x16 size, these two methods show almost the same performance.

**5. Conclusion**

We showed that our method using deep learning shows better performance than the mathematical method in the original paper **[2]**. Although our method shows better performance when the size is smaller and may show worse performance than the method in the original paper if the size is larger than 16x16, our approach to find the optimal placement and time allocation for HAP using deep learning is meaningful because there is no attempt to apply deep learning to this problem yet. There are some limits for our study. First, our study has an advantageous point for our method that it uses only 1 HAP but the method in the original paper may and commonly use more than 1 HAPs. Second, we studied with just a few conditions, 3 options for map size and 2 options for the number of WDs. So some future study should be done for many options for map size and the number of WDs, and the number of HAPs should be an additional option.

**6. References**

**[1]** Suzhi Bi, Yong Zeng, and Rui Zhang, “Wireless Powered Communication Networks: An Overview”, IEEE, available online at <https://arXiv:1508.06366>

**[2]** Suzhi Bi, Member, IEEE, and Rui Zhang, “Placement Optimization of Energy and Information Access Points in Wireless Powered Communication Networks”, IEEE Transactions on wireless communications, VOL. 15, NO. 3, MARCH 2016

**[3]** Hyungsik Ju and Rui Zhang, “Throughput Maximization in Wireless Powered Communication Networks”, available online at <https://arXiv:1304.7886v4>

**[4]** Diederik P. Kingma, Jimmy Lei Ba, “ADAM: A METHOD FOR STOCHASTIC OPTIMIZATION”, ICLR 2015, available online at <https://arXiv:1412.6980>